{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["选择题","判断题"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"选择题","index":0,"n_rows":16,"n_cols":18,"rows_kept":16,"flags":["formulas_cached_only"]}
["EXAM_QUESTION_SELECT"]
["模板说明\n1、单选题且多个得分：默认分列里的值的顺序和试题选项顺序一一对应，正确答案栏为空即可。\n2、默认分、知识点列中的逗号必选为英文逗号。\n3、多选题不支持每个选项不同得分。\n4、*号为必填项"]
["标题(*)","类型(*)","难度","默认分","解析","正确答案","选项（A）(*)","选项（B）(*)","选项（C）","选项（D）","选项（E）","选项（F）","选项（G）","选项（H）","选项（I）","选项（J）","选项（K）","选项（H）"]
["控制计划包括（）","单选题","中",4,"技术类","D","样件控制计划","试生产控制计划","生产控制计划","包括A、B、C"]
["制定控制计划的依据（）\n","多选题","中",4,"技术类","ABCD","过程流程图","FMEA","相似零件得到的经验","特殊特性"]
["控制计划应包括（ ）生产的过程输出处于控制状态","多选题","中",4,"技术类","ABCD","来料","加工","装配  ","出厂和产品运输到顾客的过程"]
["以下对控制计划描述正确的是（ ）","单选题","中",4,"技术类","C","控制计划可以根据检验指导书来制定\n \n","控制计划制定后就无需再更改\n \n","对所有受影响的操作，任何时候都应具备可供使用的控制计划\n \n","制定试生产控制计划时，因生产过程尚不稳定，可以只控制产品而不控制过程参数\n"]
["以下关于PFMEA的说法错误的是（ ）","单选题","中",4,"技术类","A","探测度分数为10时，表示“肯定能探测出来”的情况","在准备PFMEA 时，应假定所接收的材料/零件是正确的","在进行PFMEA分析时，应假定所设计的产品能够满足设计要求","FMEA 强调的是“事前”行为，而不是“事后”操作"]
["FMEA 是一种（ ）工具","单选题","中",4,"技术类","C","过程分析","问题解决","风险分析","项目策划"]
["PFMEA 分析第二步为结构分析，在分析过程工作要素时，需要考虑那些方面（ ）","多选题","中",4,"技术类","ACD","设备","原材料","间接材料","环境"]
["所谓潜在失效就意味着（ ）","单选题","中",4,"技术类","C","一定会发生","一定不会发生","不可预防","可能发生，可能不发生"]
["以下那种情况应优先采取措施（ ）","单选题","中",4,"技术类","A","S=9,O=3,D=3","S=3，O=9,D=3","S=3，O=3，D=9"]
["PFMEA 里的控制是指预防和探测（ ）的活动","多选题","中",4,"技术类","AD","失效原因","失效影响","过程功能","失效模式"]
["以下那些可以作为PFMEA的输入（）","多选题","中",4,"技术类","ABD","此项目的图纸","此项目的特殊特性清单","此项目的控制计划","此项目的过程流程图"]
["PFMEA 关于失效的影响，描述为顾客注意或体验的结果，顾客可能是（）","多选题","中",4,"技术类","ABC","公司内部后续的操作人员","外部顾客经销商","最终消费者用户","供应商"]
["在PFMEA 分析失效原因时，下列哪个失效原因的分析是正确的（）","多选题","中",4,"技术类","ABC","原材料来料时超出有效期","作业员没有搅拌均匀的情况下进行了作业","作业员没有按照作业指导书操作","设备出现故障"]

{"sheet":"判断题","index":1,"n_rows":14,"n_cols":5,"rows_kept":14,"flags":["formulas_cached_only"]}
["EXAM_QUESTION_JUDGE"]
["标题(*)","难度","默认分","解析","正确答案(*)"]
["FMEA一旦开始就是动态文件，可以根据需要进行调整","易",4,"FMEA为动态文件，根据需要实时更新 ","正确"]
["PFMEA假定所设计的产品能满足设计要求\n \n","中",4,"PFMEA假定设计满足要求","正确"]
["PFMEA不依靠改变设计来来来客服过程中的薄弱环节，因此不考虑与制造有关的产品设计特性\n \n","中",4,"PFMEA需要考虑与制造有关的产品设计特性","错误"]
["降低探测度登记最有效的措施是增加检测频次\n \n","中",4,"探测措施不变更，只改变频次，探测度不发生变化","错误"]
["开展PFMEA的主要目的是为了持续改进，预防缺陷\n","中",4,"PFMEA的目的","正确"]
["PFMEA的主要工作是生产阶段进行的\n \n","中",4,"PFMEA从DR阶段开始分析，DV前完成初版，后续持续更新","错误"]
["PFMEA假定所设计的产品能满足设计要求\n \n","中",4,"PFMEA假定设计满足要求","正确"]
["只有设计或者过程修订能够降低严重度等级\n \n","中",4,"严重度仅与设计或者过程设计有关","正确"]
["当小组开发控制计划，必须保证PFMEA的先行控制和控制计划里的控制方法一致 \n","中",4,"控制计划与PFMEA的一致性","正确"]
["过程流程图是PFMEA的输入，确定分析边界","中",4,"过程流程图是PFMEA的输入，确定分析边界","正确"]
["控制计划是由工艺部门完成","易",4,"控制计划是多功能小组共同完成","错误"]
["控制计划随着测量系统和控制方法的评价和改进而被修订","中",4,"控制计划是动态文件，当前测量和控制方法有改进时，应进行修订","正确"]